// File: mem.bmm
// datata2mem -bm this_file.bmm -bt source.bit -bd programam.mem -o b target.bit 

ADDRESS_BLOCK U_ROM RAMB4 [0x0000:0x07ff]
	BUS_BLOCK
              INST_8051/U_ROM/U_ROM0 [7:0] LOC=X1Y2;
	END_BUS_BLOCK;
	BUS_BLOCK
              INST_8051/U_ROM/U_ROM1 [7:0] LOC=X1Y1;
	END_BUS_BLOCK;
	BUS_BLOCK
              INST_8051/U_ROM/U_ROM2 [7:0] LOC=X1Y0;
	END_BUS_BLOCK;
	BUS_BLOCK
              INST_8051/U_ROM/U_ROM3 [7:0] LOC=X1Y3;
	END_BUS_BLOCK;
END_ADDRESS_BLOCK;

